**External Outputs (EOs)**

This Transactional Function point gives the user the ability to produce outputs. The results displayed are derived using data that is maintained and data that is referenced. In function point terminology the resulting display is called an External Output (EO). In accordance to the RASD documents, we have identified these points:

|  |  |  |
| --- | --- | --- |
| **EO** | **Complexity** | **FP** |
| Send password to user | Low | 4 |
| Sign up confirmation | Low | 4 |
| Show current reservation time | Low | 4 |
| Show last rides’ invoices | Average | 5 |
| Reservation confirmation | Low | 4 |
| Canceling reservation confirmation | Low | 4 |
| Navigation tips | Average | 5 |
| Cars located nearby or by specifying an address | Average | 5 |
| Money saving option navigation tips | Average | 5 |
| Almost empty battery notification | Average | 5 |
| Non-uniform cars’ distribution notification | High | 7 |
| Technical issue notification | High | 7 |
| Driver recognition confirmation | Low | 4 |
| Engine deactivation notification | Low | 4 |
| 8 hours’ driving time exceeded notification | Low | 4 |
| Tot. |  | 71 |